|  |  |  |  |
| --- | --- | --- | --- |
|  | | |  |
| **Annexure MRTS68.1** | | |
| **Dynamic Testing of Piles** | | |
|  | | |
| **Specific Contract Requirements** | | |
|  | | |
| **Contract Number** | |  |
|  | | | |
| Note: | Clause references within brackets in this Annexure refer to Clauses in the parent Technical Specification MRTS68 unless otherwise noted. | | |

|  |  |  |
| --- | --- | --- |
| Number of piles to be dynamically tested (Clause 6) | | |
|  | The number of piles to be dynamically tested shall be |  |

|  |  |
| --- | --- |
| Location of piles to be dynamically tested (Clause 6) | |
|  | Piles in the following locations shall be dynamically tested. Where no location are stated below, piles to be tested will be nominated by the Administrator.  The number of piles to be dynamically tested may be increased by the requirements of MRTS65 or MRTS66 where the Contractor elects to use a different hammer than the design hammer. |
|  |  |

|  |  |
| --- | --- |
| Supplementary requirements (Clause 12) | |
|  | The following supplementary requirements shall apply. |
|  |  |