**Checklist – CAC061M  
Inspection – Fibre-Reinforced Concrete Pipes – MRTS26**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Contractor** |  | **Date** |  | **Review No.** |  |
| **Contract No.** |  | **Project No.** |  | **Project Name** |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Unit Numbers** |  | **Unit Types** |  | **Date Manufactured** |  |

| Reference | Requirements | Addressed | Comments/Observations |
| --- | --- | --- | --- |
| MRTS26 Cl. 6  AS 4139 Cl. 6 | Registration of materials |  |  |
| MRTS26 Cl. 10  AS 4139 Cl. 12 | Marking & identification of product |  |  |
| MRTS25 Cl. 7c  AS 4139 Cl. 9 | Surface finish |  |  |
| MRTS26 Cl. 7c  AS 4139 Cl. 10 | Dimensional check - 1/50 (each size/class) |  |  |
| MRTS26 Cl. 7b | Load testing - 1/100 (each size/class) |  |  |
| AS 4139 Cl. 13 | Stacking and storage |  |  |
|  | Were repairs carried out satisfactorily? |  |  |

*Delete below section if not required*

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Audited by: |  | |  | |  | |
| Name |  | Signature |  | Date |  |