|  |  |
| --- | --- |
|  |  |
| **Annexure MRS07C.1 (July 2024)** |
| **Insitu Stabilised Pavements using Foamed Bitumen** |
|  |
| **Specific Contract Requirements** |
|  |
| **Contract Number**  |  |
|  |
| Note: | Clause references within brackets in this Annexure refer to Clauses in the parent Specification MRS07C unless otherwise noted. |

|  |
| --- |
| Utilisation of a rejected lot for a reduced level of service (Table 3.1) |
|  | The maximum road roughness value (Rₘ) |  | m/km |
|  | If no value is given, it shall equal Rₛ + 0.76 m/km, where Rₛ is defined in MRTS07C. |

|  |
| --- |
| Reduced value for insufficient thickness of stabilised layer (Clause 3.2.5) |
|  | Reduced value payment for insufficient thickness of stabilised layer shall apply | Yes |  | No |  |
|  | If no indication is given, the reduced value payment shall apply. |

|  |
| --- |
| Additional payment for a higher standard of surface evenness (Clause 4.1) |
|  | An additional payment for a higher standard of surface evenness shall apply | Yes |  | No |  |
|  | If no indication is given, the additional payment shall not apply. |