|  |  |
| --- | --- |
|  |  |
| **Annexure MRTS10.1 (July 2020)** |
| **Plant-Mixed Lightly Bound Pavements** |
|  |
| **Specific Contract Requirements** |
|  |
| **Contract Number**  |  |
|  |
| Note: | Clause references within brackets in this Annexure refer to Clauses in the parent Technical Specification MRTS10 unless otherwise noted. |
| Construction requirementsPaving equipment – lightly bound base (Clause 8.2.1.4) |
|  | A self-propelled spreading machine (paver) is required: | Yes |  | No |  |
|  | If no indication is given, plant-mixed lightly bound base shall be constructed using a self-propelled spreading machine (that is, a paver). |

|  |
| --- |
| Paving equipment – lightly bound subbase (Clause 8.2.1.4) |
|  | A self-propelled spreading machine (paver) is required: | Yes |  | No |  |
|  | If no indication is given, plant-mixed lightly bound subbase shall be constructed using either a grader or paver. |

|  |
| --- |
| Straight-edge tolerances applicable on layers other than the final layer (Clause 8.3.6) |
|  | In addition to the final layer of lightly bound base, the specified requirement for deviation from a straight-edge shall also apply to the following layers. |
| Material Type | Additional Layer to be Tested |
|  |  |
|  |  |
| If no indication is given, the requirement for deviation from a straight-edge shall apply to the final (uppermost) layer of lightly bound base only. |

|  |
| --- |
| Road roughness (Clause 8.3.7) |
|  | The maximum road roughness shall be (Rs) |  | m/km |
|  | If no indication is given, the requirements shall be 2.31. |

|  |
| --- |
| Trafficking during construction (Clause 8.2.11) |
|  | The following requirements for trafficking during construction shall apply. |
| Layer | Requirement |
|  |  |
|  |  |

|  |
| --- |
| Supplementary requirements (Clause 10) |
|  | The following supplementary requirements shall apply. |
|  |  |