|  |  |
| --- | --- |
|  |  |
| **Annexure MRTS58.1 (July 2024)** |
| **Geosynthetics for Subgrade and Pavement Reinforcement** |
|  |
| **Specific Contract Requirements** |
|  |
| **Contract Number**  |  |
|  |
| Note: | Clause references within brackets in this Annexure refer to Clauses in the parent Technical Specification MRTS58 unless otherwise noted. |
| Details of the geosynthetic (Clause 6.1.1)When considering the geosynthetic type, refer to Clause 6.1.1 for selection guidance. |
| Reference location |  |  |
| Nominated geosynthetic product †1 |  |  |
| Nominated geosynthetic type †2 |  |  |
| †1The nominated geosynthetic product shall be *geogrid* or *geocomposite*. If no indication is given above or shown in the Drawings, it shall be nominated by the Contractor and be *geogrid* or *geocomposite*.†1The nominated geosynthetic type shall be either *Type 1*or *Type 2*. If no indication is given above or shown in the Drawings, it shall be nominated by the Contractor and be *Type 1*or *Type 2*. |
| Supplementary requirements (Clause 10) |
|  | The following supplementary requirements shall apply. |
|  |  |