|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | |  | |
| **Annexure MRTS104.1 (July 2021)** | | | | | |
| **Retarding Pavement Reflective Cracking using Asphalt Geosynthetics** | | | | | |
|  | | | | | |
| **Specific Contract Requirements** | | | | | |
|  | | | | | |
| **Contract Number** | | |  | | |
|  | | | | | | | |
| Note: | | Clause references within brackets in this Annexure refer to Clauses in the parent Technical Specification MRTS104 unless otherwise noted. | | | | | |
| Details of the asphalt geosynthetic (Clause 7.2) When considering the asphalt geosynthetic materials and types, refer to Clause 1 for descriptions, Clause 2 for definition of terms, and, Clauses 6.1, 6.2 and 6.3 for selection guidance. | | | | | | | |
| Reference location | | | |  |  | | |
| Nominated asphalt geogrid material †1 | | | |  |  | | |
| Nominated asphalt geosynthetic type †2 | | | |  |  | | |
| †1 The nominated asphalt geogrid material shall be *glass fibre* or *polymeric*. If no indication is given above or shown on the Drawings, *glass fibre* or *polymeric* shall be nominated.  †2 The nominated asphalt geosynthetic type shall be *geogrid without geotextile backing* or *geogrid with geotextile backing*. If no indication is given above or shown on the Drawings, *geogrid with geotextile backing* shall be nominated. | | | | | | | |
| Supplementary requirements (Clause 11) | | | | | | |
|  | The following supplementary requirements shall apply. | | | | | |
|  |  | | | | | |