|  |  |  |  |
| --- | --- | --- | --- |
|  | | |  |
| **Annexure MRTS74.1 (November 2023)** | | |
| **Supply and Erection of Prestressed Concrete Deck Units, Kerb Units and Winged Planks** | | |
|  | | |
| **Specific Contract Requirements** | | |
|  | | |
| **Contract Number** | |  |
|  | | | |
| Note: | Clause references within brackets in this Annexure refer to Clauses in the parent Technical Specification MRTS74 unless otherwise noted. | | |

|  |  |
| --- | --- |
| Proprietary grouting products for grouting of transverse stressing holes – (Clauses 6.3.1 and 8.7) The following products are registered for use. | |
|  |  |
| Cementitious grout for filling up Holding Down Bolts (Clauses 6.3.2 and 9.1) The following products are registered for use. | |
|  |  |
| Epoxy paste for seating of prestressed concrete deck and kerb units – Transport and Main Roads Registered Products (Clauses 6.1, 6.4 and 7.3.3) The following products are registered for use. | |
|  |  |
| Surface tolerant epoxy for cut off lifting hoop anchors, cast in lifting anchor and anchorage protection – Transport and Main Roads Registered Products (Clauses 6.1, 10.3, 10.4 and 11.1) The following products are registered for use. | |
|  |  |
| Wet-to-dry epoxy for transverse stressing anchorage recesses – Transport and Main Roads Registered Products (Clauses 6.1 and 11.2) The following products are registered for use. | |
|  |  |
| Supplementary requirements (Clause 13) The following supplementary requirements shall apply. | |
|  |  |